2/13/2017

LINCOLN II +

Features.

The same as LINCOLN II V3 plus:

-The 12meter band has been added (24,880Mhz to 24,980Mhz)

-The key “CH19/9” has been replaced by “Emergency Channel 1 and 2” Programmable by the user menu.

-The “+” printed on the front panel of the radio

-A little more HF output power 35W PEP SSB(+) instead of 31W PEP SSB and 35W FM(+) instead of 28W for AM the same 12W RMS→48WPEP

Some improvements on existing functions of the current LINCOLN II:

-Audio volume behavior improved.

-Mike behavior improved.

-Echo level fixed and improved.

-RF Gain behavior improved.

-CTCSS code possible only for TX mode.

The user can use the software (computer connected by USB cord) and allows the user to rename the “BAND name, the emergency channels and other personalization features.